Bergman 1-100 LVT-4 (armed,armoured version)

LVT-4  (2x .50cal MGs up front, 2x .30cal MGs at rear.)
LVT-4 with flat shields
LVT-4 with box shields

LVT-4 (waterline)
LVT-4 (waterline) with flat shields
LVT-4 (waterline) with box shields

LVT-4 with Polsten cannon  (cannon up front, 2x .50cal MGs in boxshields at rear.)
LVT-4 with Polsten cannon (waterline)


Polsten cannon has a strong-enough spigot that it doesn't require gluing.
For the MGs: clip the location spigot short, shave spigot to fit, and glue in place.
Note that if you wish to carry a Jeep, the .30cal MGs need to be glued swung out of the way of the cargo area.