                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2492121
ABSDBS-8" ver. 0.71b by Fatalik is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

My 200/1000 newton telescope from ABS which weights only 5,5kg  
 a regular 200x200mm printer is sufficient for the OTA and  mount.
https://youtu.be/rU0g6_gWuTk

Construction designed for the HC-1 focuser which weights only 62grams and don't jamming in the cold which frequently occurs for the threaded helix focusers.  (may be used another focuser but this requeres focuser-platform redesign)

the list and the number of printed items in a text file

Also this construction requires a bunch of bolts and nuts, M4 and M5, three good and hard springs (with diameter of M5 bolts), 8 aluminum tubes of diameter 12 mm
and length of ~870mm*, 6 bearings with diameter 16mm bore 5mm, spider with secondary mirror , main mirror, focuser.

https://youtu.be/r6JPN2v9uLg
https://youtu.be/1REHZZvOI_0 Assembly absdbs-8" =)

 fb: https://www.facebook.com/profile.php?id=100003787244126
 vk: https://vk.com/homemadedob

In the comments ask a question what kind of mirror will do. Only parabolic not spherical, on Ali Express often sell spherical mirror , it is necessary to clarify this point
I'm not very well versed in trading platforms but I think on eBay you can buy the right mirror =)
I just did - I bought a used tube Newtonian without a mount (OTA) and took out of it :)
I have a set of 203mm primary mirror with a focal length of 1000mm and the secondary mirror 52mm small axis. You can take the 200mm mirror with a large (or smaller) focal length, this will require to add a length of pipe and add another counterweight. The size of the required secondary mirror can count "calculator telescope Newton" or that it is easier to ask there where you will take a main mirror which is secondary to his suit.
Also on this site there are many variants of pointer holders, focuser and other details. I'll try to print them out and add in the description links to them =) why make a new version of what already is there.
My text can be write errors i'm using an automatic translator

Useful additions:

Laser Mount for Telescopes by nfhslugger
Published on December 24, 2014
www.thingiverse.com/thing:608140
Telescope Dovetail Base by ahicktiger
Published on February 23, 2017
www.thingiverse.com/thing:2132355
M5 Thumbscrew by CD4017
Published on July 8, 2017
www.thingiverse.com/thing:2424613

Focuser!!! for ABSDBS from Marcelo Bastos =)
 https://www.thingiverse.com/thing:2658607

ABSDBS number of printing parts:
name      count
dob-ear-r300-part-1			2
dob-ear-r300-part-2			2
dob-ear-r300-part-3			2
dob-ear-spacer				4
focuser-plate				1
fold-cover-A				2
fold-cover-B				2
main-box-part-A				2
main-box-part-B				2
mirror-cell-core			1
mirror-cell-leg				3
mirror-cell-clip			3
mount-ring-top-A			2
mount-ring-top-B			2
NEW07b-mount-support-ring-part-1	1
NEW07b-mount-support-ring-part-2	1 
NEW07b-mount-support-ring-part-3	1 
NEW07b-mount-support-ring-part-4-fix	1 
spacer-top-rings-A			2
spacer-top-rings-B			2
spider-clamp				4
top-ring-part				8
tube-clip				16
ear-slot-rev5				2
ear-slot-part2-rev5			2
fixation-conterweight			1
counterweight mount			1
mount-stand				3
fold-cover-fixation-part-1		2
fold-cover-fixation-part-2		2

# Print Settings

Infill: 20

Notes: 
 a regular 200x200mm printer is sufficient for the OTA and  mount.