dob-ear-r300-part-1			2
dob-ear-r300-part-2			2
dob-ear-r300-part-3			2
dob-ear-spacer				4
focuser-plate				1
fold-cover-A				2
fold-cover-B				2
main-box-part-A				2
main-box-part-B				2
mirror-cell-core			1
mirror-cell-leg				3
mirror-cell-clip			3
mount-ring-top-A			2
mount-ring-top-B			2
NEW07b-mount-support-ring-part-1	1
NEW07b-mount-support-ring-part-2	1 
NEW07b-mount-support-ring-part-3	1 
NEW07b-mount-support-ring-part-4-fix	1 
spacer-top-rings-A			2
spacer-top-rings-B			2
spider-clamp				4
top-ring-part				8
tube-clip				16
ear-slot-rev5				2
ear-slot-part2-rev5			2
fixation-conterweight			1
counterweight mount			1
mount-stand				3
fold-cover-fixation-part-1		2
fold-cover-fixation-part-2		2
___________________________________________
aluminum tubes of diameter 12 mm
and length of ~870ٌٌ* 			8
bearings with diameter 16mm bore 5mm	6
main mirror 8"				1 :)
spider and sec. mirror 			1
focuser HC-1** (weight 62 grams!!!)	1
___________________________________________
**(the area under the 
focuser drawn for حر-1)
*(tubes long depends on the focuser
and the focuser landing)